These graphs provided are testing the LEDs with photoresistor and not upgraded TX or RX circuit. The graphs below show the Photoresistor Analog Values along the Y-axis and the number of values on the X-axis. The code is designed to test 200 values so once 200 values have been read then the light stops. The titles of graphs display what values were enter in for the RGB lights. The best values of RGB would be at the brightest light level.

Graphical user interface, text, application

Description automatically generated

Graphical user interface, chart, line chart

Description automatically generated

Graphical user interface, chart

Description automatically generated

Chart, line chart

Description automatically generated

Chart, waterfall chart

Description automatically generated

Graphical user interface, text, application, email

Description automatically generated

Graphical user interface, chart, waterfall chart

Description automatically generated

The graphs below show the Photoresistor Analog Values along the Y-axis and the number of values on the X-axis. The code is designed to test 200 values so once 200 values have been read then the light stops. The graphs below show the Bright Adafruit LED with low, half, and full brightness. The values given are more consistent with the high brightness.

Table

Description automatically generated

Chart

Description automatically generated

Chart, line chart

Description automatically generated

Graphical user interface

Description automatically generated

These graphs provided are testing the LEDs with photodiode with the upgraded TX or RX circuit. The graphs below show the Photodiode Analog Values along the Y-axis and the number of values on the X-axis. The code is designed to test 200 values so once 200 values have been read then the light stops. Since I was getting crazy numbers for anything but the highest brightness level (255) there is only the room and high brightness graphs.

